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Waterborne Polyurethane Resins
PRODUCT DESCRIPTION
Waterborne polyurethane dispersion.
KEY CHARACTERISTICS
• Improves coating abrasion and scratch resistance.
• Forms a tough, elastic film.
• Good mechanical processing stability and leveling.
TECHNICAL PROPERTIES
	Appearance
	Semi-transparent liquid

	Solid Content
	±30%

	pH
	7-9

	Character
	Medium-hard


RECOMMENDED USE
Suitable for a broad range of leather, synthetic leather and microfiber (PU/PVC) finishing systems to improve overall physical performance.
STORAGE & HANDLING
Store at 5°C–40°C in sealed original packaging. The source manual states a shelf life of at least one year under these conditions. Reseal after each use, use opened material as soon as practical, protect from freezing, and mix thoroughly before use.
	Source basis: FAST Product Manual v6 supplied for this project. This sheet reproduces source-manual data for technical reference. No warranty is expressed or implied; verify current specification and test suitability before use.




FAST  富可耐   |   技术数据表
RU-3250  水性聚氨酯树脂
水性聚氨酯树脂
产品描述
水性聚氨酯分散液
主要特性
• 增进涂饰的耐磨耗和耐刮性
• 成膜坚韧有弹性
• 具有良好的机械操作稳定性、流平性
技术参数
	外观
	半透明液体

	固含量
	±30%

	pH值
	7-9

	特性
	中硬


使用建议
适用于广泛各类皮革、合成革、超纤（PU/PVC）涂饰中，以提升总体物性。
储存与使用
5℃～40℃，密封的原包装中至少可以保存一年，每次使用后，应重新将包装密封，一旦开启包装，应尽快将内装产品用完，本品必须防冻保存，使用前必须混合均匀。
	资料依据：本项目提供的 FAST《富可耐水性涂层材料 产品说明书》v6。本表按原说明书整理，仅供技术参考，不具任何保证性质；使用前请确认当前规格并预先试验其适用性。
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