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Waterborne Polyurethane Resins
PRODUCT DESCRIPTION
Waterborne aliphatic polyurethane dispersion designed to improve overall physical performance.
KEY CHARACTERISTICS
• Suitable as a mid/basecoat resin for various leather applications.
• Excellent UV resistance.
• Strong rebound.
• Forms a soft film with strong clarity.
TECHNICAL PROPERTIES
	Appearance
	Milky white liquid

	Solid Content
	±55%

	pH
	7-9


RECOMMENDED USE
Suitable for various leather, synthetic leather and microfiber (PU/PVC) coatings to improve rebound and overall physical performance.
STORAGE & HANDLING
Store at 5°C–40°C in sealed original packaging. The source manual states a shelf life of at least one year under these conditions. Reseal after each use, use opened material as soon as practical, protect from freezing, and mix thoroughly before use.
	Source basis: FAST Product Manual v6 supplied for this project. This sheet reproduces source-manual data for technical reference. No warranty is expressed or implied; verify current specification and test suitability before use.
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水性聚氨酯树脂
产品描述
水性脂肪族聚氨酯分散液，高物性能可以增加总体特性
主要特性
• 适用于各类皮革，中底涂树脂
• 特优的紫外线照射性能
• 具有很强的回弹性
• 成膜柔软，通透感强
技术参数
	外观
	乳白液体

	固含量
	±55%

	pH值
	7-9


使用建议
可广泛地使用各类皮革，合成革，超纤（PU/PVC）涂层，增加皮革的回弹性等，高物性能。
储存与使用
5℃～40℃，密封的原包装中至少可以保存一年，每次使用后，应重新将包装密封，一旦开启包装，应尽快将内装产品用完，本品必须防冻保存，使用前必须混合均匀。
	资料依据：本项目提供的 FAST《富可耐水性涂层材料 产品说明书》v6。本表按原说明书整理，仅供技术参考，不具任何保证性质；使用前请确认当前规格并预先试验其适用性。


FAST | fukenai@salesfastinter.com | WhatsApp +1 682 358 9060 | salesfastinter.com




