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Waterborne Polyurethane Foaming Resins
PRODUCT DESCRIPTION
Aromatic waterborne polyurethane foaming resin emulsion.
KEY CHARACTERISTICS
• Low-modulus, high-solids resin.
• Comfortable hand with high fullness.
• Good stability and dispersion.
• Hydrolysis and cold resistance.
TECHNICAL PROPERTIES
	Appearance
	Milky white liquid

	Solid Content
	±50%

	pH
	6-8


RECOMMENDED USE
Suitable for water-based footwear leather and dry-process base layers, providing a comfortable hand and good fullness. Dosage should be adjusted according to process conditions and formulation ratio.
STORAGE & HANDLING
Store at 5°C–40°C in sealed original packaging. The source manual states a shelf life of at least one year under these conditions. Reseal after each use, use opened material as soon as practical, protect from freezing, and mix thoroughly before use.
	Source basis: FAST Product Manual v6 supplied for this project. This sheet reproduces source-manual data for technical reference. No warranty is expressed or implied; verify current specification and test suitability before use.
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水性聚氨酯发泡树脂
产品描述
芳香族水性聚氨酯发泡树脂乳液
主要特性
• 低模量，高含量树脂
• 手感舒适，丰满度高
• 具有很好稳定性，分散性
• 耐水解，耐寒性
技术参数
	外观
	乳白色液体

	固含量
	±50%

	pH值
	6-8


使用建议
适合于水性鞋革，干法贝斯，具有很好舒适手感，丰满度好，根据工艺和配比定量。
储存与使用
5℃～40℃，密封的原包装中至少可以保存一年，每次使用后，应重新将包装密封，一旦开启包装，应尽快将内装产品用完，本品必须防冻保存，使用前必须混合均匀。
	资料依据：本项目提供的 FAST《富可耐水性涂层材料 产品说明书》v6。本表按原说明书整理，仅供技术参考，不具任何保证性质；使用前请确认当前规格并预先试验其适用性。
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