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SECTION 1  Chemical Product and Company Identification
	Product name
	Waterborne Polyurethane Resin

	Product code
	RU-3340

	Supplier
	Shanghai FAST Industrial Co., Ltd.

	Address
	Room 418, No. 1471 Gumei Road, Minhang District, Shanghai, China

	Telephone
	+86-021-34223449

	Fax
	+86-021-34222147

	Emergency telephone
	+86-021-54802120

	Email
	fastph@163.com


SECTION 2  Hazards Identification
	Most significant hazard effects
	None.

	Health hazard effects
	No adverse reactions have been recorded.

	Environmental impact
	Biodegradable; no adverse reactions have been recorded.

	Physical and chemical hazards
	Excessive contact may cause discomfort; no chemical hazard is produced.

	Main symptoms
	Inhalation: generally no adverse reaction. Contact: excessive contact may cause discomfort. Eyes: entry into the eyes may cause inflammation. Ingestion: may cause stomach discomfort.

	Hazard classification
	Treated as a general chemical.




SECTION 3  Composition / Information on Ingredients
	Mixture
	Yes

	Physical form
	Non-foaming emulsion

	Primary use
	Leather finishing emulsion


	Chemical component
	Percentage
	CAS No.

	Polyurethane resin
	28%-32%
	51852-81-4

	H2O
	70%-74%
	7732-18-5


SECTION 4  First-Aid Measures
	Inhalation
	If adverse effects occur, move the patient to fresh air.

	Skin contact
	Slowly rinse the contaminated area with water. If irritation persists, continue rinsing.

	Eye contact
	Immediately hold eyelids open and slowly rinse contaminated eyes with running water for at least 15 minutes. Where possible, rinse with normal saline without interruption. If irritation persists, continue rinsing.

	Ingestion
	If the patient is losing consciousness or is unconscious, do not give anything by mouth. If conscious, rinse the mouth thoroughly with water. Give plenty of water to dilute the chemical in the stomach. If milk is available, it may be given after water. If spontaneous vomiting occurs, lean the patient forward to reduce aspiration risk, rinse the mouth, and continue giving water.

	Most important symptoms / hazardous effects
	Harmful if swallowed.

	If discomfort occurs
	Seek medical attention immediately.

	Protection of first-aid personnel
	Not important.

	Advice to physician
	Take appropriate medical measures.




SECTION 5  Fire-Fighting Measures
	Suitable extinguishing media
	Dry chemical powder, carbon dioxide, water fog, foam. For large fires, foam or water fog spray is recommended.

	Special fire-fighting procedures
	If safe to do so, move containers away from the fire to avoid possible rupture or explosion. Spray water to cool tanks or containers exposed to fire. Isolate unignited materials and protect personnel. Apply large quantities of water fog. Personnel without protective equipment must not enter.

	Special protective equipment for firefighters
	Firefighters must wear self-contained breathing apparatus, protective firefighting clothing, and protective gloves.


SECTION 6  Accidental Release Measures
	Personal precautions
	Safety glasses and rubber gloves are recommended. Isolate the hazardous area and keep unrelated personnel out until the spill area has been completely cleaned.

	Cleanup methods
	Do not touch spilled material and prevent it from entering drains. Keep the spill area ventilated. Small spill: absorb with sand or other non-combustible material and place the absorbed material in a suitable container for waste disposal. Large spill: contain with dikes and dispose of as waste.




SECTION 7  Handling and Storage
	Safe handling
	Use suitable protective clothing. Workers should wash hands and face before eating, drinking, or smoking. Avoid contact with eyes or skin.

	Storage
	Store in the original container, protected from sunlight, in a dry, cool, and well-ventilated place. Recommended storage temperature: 5°C-40°C. Keep the container tightly closed and sealed. Do not store in unlabeled containers. Store in the original container or another approved container made of compatible material; keep sealed when not in use to extend usable storage time.


SECTION 8  Exposure Controls / Personal Protection
	Occupational exposure control
	No special ventilation requirements. Use engineering controls consistent with good industrial hygiene and safety practice. Wash hands frequently after work or during breaks.

	Eye protection
	If splashing or eye contact may occur, safety goggles or a face shield are recommended.

	Hand protection
	In accordance with good industrial practice, rubber gloves are recommended. Wash hands immediately after contact.

	Respiratory protection
	Operators should wear a dust mask. If airborne concentration is high and odor protection is required, use a suitable compliant enclosed air-filtering respirator. Filter selection must be based on known or anticipated exposure limits, product hazards, and the safe working limits of the selected respirator.

	Body protection
	Wear ordinary work clothing. Wash immediately after skin contact.

	Hygiene measures
	Avoid eye contact. Wash hands before breaks and immediately after handling the product. Contaminated work clothing should be washed before reuse. Ensure emergency eyewash and safety shower facilities are located near the work area.




SECTION 9  Physical and Chemical Properties
	Physical state
	Liquid

	pH
	7.0-9.5

	Odor
	Very low odor

	Test method
	Open cup: not checked; Closed cup: checked

	Boiling point / range
	-

	Flammability (solid, gas)
	Nonflammable

	Decomposition temperature
	-

	Explosion limits
	-

	Evaporation rate
	-

	Solubility
	Soluble in water


SECTION 10  Stability and Reactivity
	Stability
	Product is stable.

	Incompatible materials
	Do not use together with oil-based products or other incompatible materials.

	Conditions to avoid
	Extreme temperatures.

	Hazardous polymerization
	Will not occur.

	Decomposition products
	No hazardous decomposition products under correct storage and handling conditions.


SECTION 11  Toxicological Information
	Toxicological information
	This product does not yet have experimental data, but it has been evaluated under the Preparations Directive and classified for toxic hazards. Refer in detail to Section 3, including relevant hazard and safety statements.

	Acute toxicity
	-

	Irritation
	-




SECTION 12  Ecological Information
	Environmental impact
	Relevant authorities must be informed when disposing of waste. If water sources or seasonally dry streams are contaminated, the marine protection organization must be notified immediately.


SECTION 13  Disposal Considerations
	Residual waste
	Check the possibility of reuse. Product residues should be disposed of in accordance with local regulations. Empty containers or liners may retain product residues. These materials and their containers must be disposed of safely.

	Contaminated packaging
	Empty containers should be sent to an approved waste treatment facility for recycling or disposal. Product residues may remain in containers, so label warnings should still be observed even when containers are empty.


SECTION 14  Transport Information
	Transport hazard classification
	Non-dangerous goods for transport.

	Transport modes
	Sea, road, rail.

	Packaging
	Wide-mouth plastic drum.

	Special transport methods / precautions
	Non-dangerous goods. Keep dry, avoid direct sunlight, and keep away from strong acids and strong alkalis.


SECTION 15  Regulatory Information
	Use restriction
	Strictly prohibited for food and feed processing.

	Regulatory references
	Regulations on the Safety Management of Hazardous Chemicals; Detailed Rules for Implementation of the Regulations on Safety Management of Hazardous Chemicals; Regulations on the Safe Use of Chemicals in the Workplace; Classification and Labels of Common Hazardous Chemicals (GB 13690-92); Law of the People’s Republic of China on the Prevention and Control of Environmental Pollution by Solid Waste; Catalogue of Hazardous Chemicals (2015): Not listed; List of Explosive Precursor Hazardous Chemicals (2017): Not listed.




SECTION 16  Other Information
	References
	1. Chemical safety management in the workplace
2. New Handbook of Dangerous Goods Safety
3. Encyclopedia of Hazardous Chemicals Safety Technology
4. Regulations on Registration and Management of Hazardous Chemicals

	Revision note
	Revised in accordance with requirements for preparation of Safety Data Sheets for chemical products (GB/T 17519-2013; Q/YM2-2006 applied to the previous MSDS). The information provided in this document is not a product specification and does not guarantee specific properties.

	Other information
	The data recorded in this Safety Data Sheet are intended only to improve the safe use of this product and are based on the company’s current best knowledge and experience. All data are for reference only; users should determine applicability themselves. The company accepts no responsibility for damage caused by use outside normal operating conditions or under uncontrolled conditions.
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