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230  PVC Surface Treatment Agent
Water-Based Materials for PVC
PRODUCT DESCRIPTION
Medium-hard grade for PVC surface treatment, intended to improve surface smoothness, softness and hand feel.
KEY CHARACTERISTICS
• Improves surface smoothness.
• Softness with comfortable hand.
• Abrasion and scratch resistance.
TECHNICAL PROPERTIES
	Appearance
	Milky white liquid

	Solid Content
	±12%

	pH
	7-9

	Character
	Medium-hard


RECOMMENDED USE
Suitable for PVC leather surface treatment to improve smoothness and softness. Process and dosage may be adjusted according to actual requirements.
STORAGE & HANDLING
Store at 5°C–40°C in sealed original packaging. The source manual states a shelf life of at least one year under these conditions. Reseal after each use, use opened material as soon as practical, protect from freezing, and mix thoroughly before use.
	Source basis: FAST Product Manual v6 supplied for this project. This sheet reproduces source-manual data for technical reference. No warranty is expressed or implied; verify current specification and test suitability before use.
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230  PVC表面处理剂
PVC专用水性材料
产品描述
中硬型，适用于PVC表面处理，提高革面平滑性，柔软性，手感舒适。
主要特性
• 提高革面平滑性
• 柔软性，手感舒适
• 耐磨耐刮性
技术参数
	外观
	乳白色液体

	固含量
	±12%

	pH值
	7-9

	特性
	中硬


使用建议
适用于PVC革表面处理，提高革面平滑性，柔软性，可根据实际需求调整工艺和用量。
储存与使用
5℃～40℃，密封的原包装中至少可以保存一年，每次使用后，应重新将包装密封，一旦开启包装，应尽快将内装产品用完，本品必须防冻保存，使用前必须混合均匀。
	资料依据：本项目提供的 FAST《富可耐水性涂层材料 产品说明书》v6。本表按原说明书整理，仅供技术参考，不具任何保证性质；使用前请确认当前规格并预先试验其适用性。
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