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632  Microfiber Leather Printing Emulsion
Water-Based Printing Materials
PRODUCT DESCRIPTION
Designed for high-density microfiber leather using a penetrative printing process in which the printing paste penetrates the microfiber layer, followed by surface film printing. The high-density substrate provides strong stability, abrasion resistance and flex resistance.
KEY CHARACTERISTICS
• Excellent abrasion and flex resistance; the printed layer resists delamination under repeated bending.
• No cracking with excellent breathability.
• Delicate hand with excellent dry/wet rub resistance.
• High color intensity with good long-term color stability.
TECHNICAL PROPERTIES
	Appearance
	Milky white liquid

	Solid Content
	±22%

	pH
	6-8


RECOMMENDED USE
Suitable for high-end footwear uppers, luggage, premium furniture, sofas, sports-equipment accessories and leather gifts.
STORAGE & HANDLING
Store at 5°C–40°C in sealed original packaging. The source manual states a shelf life of at least one year under these conditions. Reseal after each use, use opened material as soon as practical, protect from freezing, and mix thoroughly before use.
	Source basis: FAST Product Manual v6 supplied for this project. This sheet reproduces source-manual data for technical reference. No warranty is expressed or implied; verify current specification and test suitability before use.
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632  超纤印花乳液
水性印花专用材料
产品描述
以高密度超细纤维超纤革为基材，采用渗透式印花工艺，浆料渗入超纤纤维层，表面覆膜印花，稳定性更强，基材密度高，耐磨抗折，优质印花材料。
主要特性
• 超强耐磨，耐曲折，反复弯折印花层无脱落
• 无裂纹，透气性极佳
• 手感细腻，耐干湿擦性能优异
• 色泽度高，长期使用不发花，不变色
技术参数
	外观
	乳白色液体

	固含量
	±22%

	pH值
	6-8


使用建议
适用于高端鞋材鞋面，箱包，高档家具，沙发，运动器材配饰，皮具礼品等。
储存与使用
5℃～40℃，密封的原包装中至少可以保存一年，每次使用后，应重新将包装密封，一旦开启包装，应尽快将内装产品用完，本品必须防冻保存，使用前必须混合均匀。
	资料依据：本项目提供的 FAST《富可耐水性涂层材料 产品说明书》v6。本表按原说明书整理，仅供技术参考，不具任何保证性质；使用前请确认当前规格并预先试验其适用性。
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