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L-66  Wetting Agent
Water-Based Additives
PRODUCT DESCRIPTION
Dry-process additive.
KEY CHARACTERISTICS
• Improves leather softness, lubrication and color development. Application: coating wetting.
TECHNICAL PROPERTIES
	Solid Content
	±50%

	Type
	Dry-process additive


RECOMMENDED USE
Improves leather softness, lubrication and color development. Application: coating wetting.
STORAGE & HANDLING
Store at 5°C–40°C in sealed original packaging. The source manual states a shelf life of at least one year under these conditions. Reseal after each use.
	Source basis: FAST Product Manual v6 supplied for this project. This sheet reproduces source-manual data for technical reference. No warranty is expressed or implied; verify current specification and test suitability before use.
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L-66  润湿剂
水性助剂
产品描述
干法助剂
主要特性
• 改善皮革的柔软性、提高润滑性和展色性。应用：涂层润湿。
技术参数
	固含量
	±50%

	类型
	干法助剂


使用建议
改善皮革的柔软性、提高润滑性和展色性。应用：涂层润湿。
储存与使用
5℃～40℃，密封的原包装中至少可以保存一年，每次使用后应重新密封。
	资料依据：本项目提供的 FAST《富可耐水性涂层材料 产品说明书》v6。本表按原说明书整理，仅供技术参考，不具任何保证性质；使用前请确认当前规格并预先试验其适用性。
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