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PU-3115  Skin-Feel Surface Treatment Agent
Water-Based Surface Treatment Materials
PRODUCT DESCRIPTION
A water-based matte surface-treatment agent with excellent flex and abrasion resistance. It provides a soft, silky and full hand with a matte effect on leather, maintains performance after high-temperature ironing, and can achieve improved dry and wet rub resistance when used with a crosslinker.
TECHNICAL PROPERTIES
	Appearance
	Milky white liquid

	Solid Content
	±17%

	Ionicity
	Anionic


RECOMMENDED USE
Suitable for surface treatment of sofa leather, sheepskin garment leather, footwear uppers and PU/PVC synthetic leather. A crosslinker may be added to improve dry/wet rub resistance.
STORAGE & HANDLING
Store at 5°C–40°C in sealed original packaging. The source manual states a shelf life of at least one year under these conditions. Reseal after each use, use opened material as soon as practical, protect from freezing, and mix thoroughly before use.
	Source basis: FAST Product Manual v6 supplied for this project. This sheet reproduces source-manual data for technical reference. No warranty is expressed or implied; verify current specification and test suitability before use.
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PU-3115  肤感表处剂
水性表面处理材料
产品描述
本品水性消光表处剂，产品优异耐曲折、耐磨耗，经使用在皮革上有绵软，具有丝滑及其在皮上有丰满度，而且有不错的消光效果，经过高温烫革对皮本身不影响，加入交联剂又增强耐干湿擦。
技术参数
	外观
	乳白色液体

	固含量
	±17%

	离子性
	阴离子


使用建议
适用于沙发革、羊皮服装、鞋面革以及合成革（PU，PVC）等表面处理。加入交联剂可增强耐干湿擦性能。
储存与使用
5℃～40℃，密封的原包装中至少可以保存一年，每次使用后，应重新将包装密封，一旦开启包装，应尽快将内装产品用完，本品必须防冻保存，使用前必须混合均匀。
	资料依据：本项目提供的 FAST《富可耐水性涂层材料 产品说明书》v6。本表按原说明书整理，仅供技术参考，不具任何保证性质；使用前请确认当前规格并预先试验其适用性。
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