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PU-3116  Smooth-Feel Surface Treatment Agent
Water-Based Surface Treatment Materials
PRODUCT DESCRIPTION
A water-based matte surface-treatment agent with excellent flex, abrasion and scratch resistance. It provides a smooth, soft hand and retains a matte gloss after high-temperature ironing. A crosslinker may be used to improve abrasion and weather resistance.
TECHNICAL PROPERTIES
	Appearance
	Milky white liquid

	Solid Content
	±17%

	Ionicity
	Anionic


RECOMMENDED USE
Suitable for surface treatment of sofa leather, sheepskin garment leather, luggage and PU/PVC synthetic leather. A crosslinker may be added to improve abrasion and weather resistance.
STORAGE & HANDLING
Store at 5°C–40°C in sealed original packaging. The source manual states a shelf life of at least one year under these conditions. Reseal after each use, use opened material as soon as practical, protect from freezing, and mix thoroughly before use.
	Source basis: FAST Product Manual v6 supplied for this project. This sheet reproduces source-manual data for technical reference. No warranty is expressed or implied; verify current specification and test suitability before use.
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PU-3116  平滑表处剂
水性表面处理材料
产品描述
本品水性消光表处剂，具有优异耐曲折性，耐磨抗刮性，经使用皮革上有平滑、柔软绵感，经过高温烫革也处于哑光光泽。赋予良好的消光性，加入交联剂增加耐磨、耐候性。
技术参数
	外观
	乳白色液体

	固含量
	±17%

	离子性
	阴离子


使用建议
适用于沙发革、羊皮服装、箱包和合成革（PU，PVC）等表面处理。加入交联剂可增加耐磨、耐候性。
储存与使用
5℃～40℃，密封的原包装中至少可以保存一年，每次使用后，应重新将包装密封，一旦开启包装，应尽快将内装产品用完，本品必须防冻保存，使用前必须混合均匀。
	资料依据：本项目提供的 FAST《富可耐水性涂层材料 产品说明书》v6。本表按原说明书整理，仅供技术参考，不具任何保证性质；使用前请确认当前规格并预先试验其适用性。
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