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PU-326  Waxy-Feel Surface Treatment Agent
Water-Based Surface Treatment Materials
PRODUCT DESCRIPTION
Waterborne aliphatic matte polyurethane emulsion.
KEY CHARACTERISTICS
• Excellent softness.
• Matte gloss level.
• Good fullness with a pronounced waxy feel.
• Weather and light resistance.
TECHNICAL PROPERTIES
	Appearance
	Milky white liquid

	Solid Content
	±10%

	pH
	7-9


RECOMMENDED USE
Mainly used on PU and PVC synthetic leather surface coatings. A crosslinker may be added to achieve higher physical performance.
STORAGE & HANDLING
Store at 5°C–40°C in sealed original packaging. The source manual states a shelf life of at least one year under these conditions. Reseal after each use, use opened material as soon as practical, protect from freezing, and mix thoroughly before use.
	Source basis: FAST Product Manual v6 supplied for this project. This sheet reproduces source-manual data for technical reference. No warranty is expressed or implied; verify current specification and test suitability before use.




FAST  富可耐   |   技术数据表
PU-326  蜡感表处剂
水性表面处理材料
产品描述
水性脂肪族聚氨酯消光乳液
主要特性
• 柔软性优秀
• 哑光的光泽度
• 丰满度好，蜡感强
• 耐候性、耐光性
技术参数
	外观
	乳白色液体

	固含量
	±10%

	pH值
	7-9


使用建议
主要用于合成革（PU和PVC）表面涂层。通过添加交联剂，以获取更高物性。
储存与使用
5℃～40℃，密封的原包装中至少可以保存一年，每次使用后，应重新将包装密封，一旦开启包装，应尽快将内装产品用完，本品必须防冻保存，使用前必须混合均匀。
	资料依据：本项目提供的 FAST《富可耐水性涂层材料 产品说明书》v6。本表按原说明书整理，仅供技术参考，不具任何保证性质；使用前请确认当前规格并预先试验其适用性。
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