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PU-338  Waterborne High-Gloss Patent-Leather Surface Treatment Agent
Water-Based Surface Treatment Materials
PRODUCT DESCRIPTION
Water-based high-gloss patent-leather surface-treatment emulsion.
KEY CHARACTERISTICS
• Good film formation and strong bonding.
• Excellent cold, hydrolysis and aging resistance.
• High gloss and excellent clarity; supports printing operations.
TECHNICAL PROPERTIES
	Appearance
	Transparent liquid

	Solid Content
	±30%

	pH
	6-8


RECOMMENDED USE
Suitable as a high-gloss patent-leather surface-treatment agent for synthetic leather.
STORAGE & HANDLING
Store at 5°C–40°C in sealed original packaging. The source manual states a shelf life of at least one year under these conditions. Reseal after each use, use opened material as soon as practical, protect from freezing, and mix thoroughly before use.
	Source basis: FAST Product Manual v6 supplied for this project. This sheet reproduces source-manual data for technical reference. No warranty is expressed or implied; verify current specification and test suitability before use.
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PU-338  水性高光油皮表处剂
水性表面处理材料
产品描述
水性高光油皮表处剂乳液
主要特性
• 成膜性好，黏结牢固
• 具有优异的耐寒，耐水解，耐老化性能
• 产品亮度高，透度优异，支持印刷作业
技术参数
	外观
	透明液体

	固含量
	±30%

	pH值
	6-8


使用建议
适用于表面合成革表面,亮面油皮处理剂。
储存与使用
5℃～40℃，密封的原包装中至少可以保存一年，每次使用后，应重新将包装密封，一旦开启包装，应尽快将内装产品用完，本品必须防冻保存，使用前必须混合均匀。
	资料依据：本项目提供的 FAST《富可耐水性涂层材料 产品说明书》v6。本表按原说明书整理，仅供技术参考，不具任何保证性质；使用前请确认当前规格并预先试验其适用性。
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