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PU-348  Waterborne Gloss Surface Treatment Agent
Water-Based Surface Treatment Materials
PRODUCT DESCRIPTION
Water-based gloss surface-treatment emulsion.
KEY CHARACTERISTICS
• Anionic water-based PU material.
• Smooth, comfortable hand with clear film formation.
• High gloss.
TECHNICAL PROPERTIES
	Appearance
	Semi-transparent liquid

	Solid Content
	±30%

	pH
	7-9


RECOMMENDED USE
Suitable as a gloss surface-treatment agent for PU garment leather and for hot-ironing gloss-finishing operations.
STORAGE & HANDLING
Store at 5°C–40°C in sealed original packaging. The source manual states a shelf life of at least one year under these conditions. Reseal after each use, use opened material as soon as practical, protect from freezing, and mix thoroughly before use.
	Source basis: FAST Product Manual v6 supplied for this project. This sheet reproduces source-manual data for technical reference. No warranty is expressed or implied; verify current specification and test suitability before use.
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PU-348  水性亮面处理剂
水性表面处理材料
产品描述
水性亮面表处剂乳液
主要特性
• 阴离子型水性PU材质
• 手感滑爽舒适，成膜通透
• 高光泽度
技术参数
	外观
	半透明液体

	固含量
	±30%

	pH值
	7-9


使用建议
适用于PU服装革表面亮面处理剂，可用于烫亮处理作业。
储存与使用
5℃～40℃，密封的原包装中至少可以保存一年，每次使用后，应重新将包装密封，一旦开启包装，应尽快将内装产品用完，本品必须防冻保存，使用前必须混合均匀。 五、水性助剂 储存方法：5℃～40℃，密封的原包装中至少可以保存一年，每次使用后应重新密封。
	资料依据：本项目提供的 FAST《富可耐水性涂层材料 产品说明书》v6。本表按原说明书整理，仅供技术参考，不具任何保证性质；使用前请确认当前规格并预先试验其适用性。
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