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RU-3270  Waterborne Aliphatic Polyurethane Resin
Waterborne Polyurethane Resins
PRODUCT DESCRIPTION
Waterborne aliphatic polyurethane dispersion.
KEY CHARACTERISTICS
• Good overall performance.
• Excellent light and solvent resistance.
• Improves abrasion resistance and overall physical performance.
• Suitable for migration-resistant mid/base coating applications.
TECHNICAL PROPERTIES
	Appearance
	Semi-transparent liquid

	Solid Content
	±30%

	pH
	7-9

	Character
	Medium-hard


RECOMMENDED USE
Suitable for leather, synthetic leather, microfiber leather and related coatings to improve overall physical performance, including abrasion resistance and migration resistance on PU/PVC systems.
STORAGE & HANDLING
Store at 5°C–40°C in sealed original packaging. The source manual states a shelf life of at least one year under these conditions. Reseal after each use, use opened material as soon as practical, protect from freezing, and mix thoroughly before use.
	Source basis: FAST Product Manual v6 supplied for this project. This sheet reproduces source-manual data for technical reference. No warranty is expressed or implied; verify current specification and test suitability before use.




FAST  富可耐   |   技术数据表
RU-3270  水性脂肪族聚氨酯树脂
水性聚氨酯树脂
产品描述
水性脂肪族聚氨酯分散液
主要特性
• 综合性能良好
• 特优耐光性、耐溶剂性
• 可增进耐磨性、高物性
• 适合于中底涂饰耐色吐移性
技术参数
	外观
	半透明液体

	固含量
	±30%

	pH值
	7-9

	特性
	中硬


使用建议
适用于各类皮革，合成革、超纤、涂层等。增加涂饰高物性能，提高各类皮革（PU、PVC），耐磨性，耐迁移等。
储存与使用
5℃～40℃，密封的原包装中至少可以保存一年，每次使用后，应重新将包装密封，一旦开启包装，应尽快将内装产品用完，本品必须防冻保存，使用前必须混合均匀。
	资料依据：本项目提供的 FAST《富可耐水性涂层材料 产品说明书》v6。本表按原说明书整理，仅供技术参考，不具任何保证性质；使用前请确认当前规格并预先试验其适用性。
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