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RU-3350  Waterborne Aliphatic Polyurethane Resin
Waterborne Polyurethane Resins
PRODUCT DESCRIPTION
Aliphatic polyurethane dispersion.
KEY CHARACTERISTICS
• Good overall performance.
• Excellent cold and flex resistance.
• Very strong UV resistance.
• Good drum-tumbling resistance and embossing/shape-setting performance.
• Uniform appearance with excellent covering performance.
TECHNICAL PROPERTIES
	Appearance
	Semi-transparent liquid

	Solid Content
	±30%

	pH
	7-9

	Character
	Medium-hard


RECOMMENDED USE
Suitable for a wide range of leather coating systems (PU/PVC) and general mid/basecoat formulations.
STORAGE & HANDLING
Store at 5°C–40°C in sealed original packaging. The source manual states a shelf life of at least one year under these conditions. Reseal after each use, use opened material as soon as practical, protect from freezing, and mix thoroughly before use.
	Source basis: FAST Product Manual v6 supplied for this project. This sheet reproduces source-manual data for technical reference. No warranty is expressed or implied; verify current specification and test suitability before use.
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RU-3350  水性脂肪族聚氨酯树脂
水性聚氨酯树脂
产品描述
脂肪族聚氨酯分散乳液
主要特性
• 具有良好的综合性能
• 特优的耐寒性，耐曲挠性
• 耐紫外线照射性特强
• 良好的耐摔鼓性压花定型
• 外观均匀，并具有各种特优遮盖性
技术参数
	外观
	半透明液体

	固含量
	±30%

	pH值
	7-9

	特性
	中硬


使用建议
可广泛地使用各类皮革（PU，PVC）涂层中，也可以使用于一般中底涂配方。
储存与使用
5℃～40℃，密封的原包装中至少可以保存一年，每次使用后，应重新将包装密封，一旦开启包装，应尽快将内装产品用完，本品必须防冻保存，使用前必须混合均匀。
	资料依据：本项目提供的 FAST《富可耐水性涂层材料 产品说明书》v6。本表按原说明书整理，仅供技术参考，不具任何保证性质；使用前请确认当前规格并预先试验其适用性。
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