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RU-3370  Aliphatic Polyurethane Resin
Waterborne Polyurethane Resins
PRODUCT DESCRIPTION
Aliphatic polyurethane dispersion.
KEY CHARACTERISTICS
• Excellent cold and flex resistance.
• Excellent embossing and flattening performance.
• Good covering, uniformity and filling performance.
• Forms a clear, non-tacky film with excellent water resistance.
• Excellent UV resistance.
TECHNICAL PROPERTIES
	Appearance
	Transparent liquid

	Solid Content
	±30%

	pH
	7-9

	Character
	Medium-hard


RECOMMENDED USE
For producing natural-looking finishes on leather, PU/PVC sofa leather, microfiber leather, footwear uppers and luggage leather, in both base and top layers.
STORAGE & HANDLING
Store at 5°C–40°C in sealed original packaging. The source manual states a shelf life of at least one year under these conditions. Reseal after each use, use opened material as soon as practical, protect from freezing, and mix thoroughly before use.
	Source basis: FAST Product Manual v6 supplied for this project. This sheet reproduces source-manual data for technical reference. No warranty is expressed or implied; verify current specification and test suitability before use.
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RU-3370  脂肪族聚氨酯树脂
水性聚氨酯树脂
产品描述
脂肪族聚氨酯分散乳液
主要特性
• 特优的耐寒性、曲挠性
• 特优的压花性和压平性能极佳
• 良好的遮盖性、均匀性、填充性
• 成膜通透且不发黏，耐水性特优
• 耐紫外线照射性极好
技术参数
	外观
	透明液体

	固含量
	±30%

	pH值
	7-9

	特性
	中硬


使用建议
使用以生产外观自然的涂饰，适合于（皮革，PU，PVC）沙发革、超纤、鞋面革、箱包底层和面层中。
储存与使用
5℃～40℃，密封的原包装中至少可以保存一年，每次使用后，应重新将包装密封，一旦开启包装，应尽快将内装产品用完，本品必须防冻保存，使用前必须混合均匀。
	资料依据：本项目提供的 FAST《富可耐水性涂层材料 产品说明书》v6。本表按原说明书整理，仅供技术参考，不具任何保证性质；使用前请确认当前规格并预先试验其适用性。
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