
RU-6880
Matte Polyurethane Resin (Polycarbonate)								

Characteristics:
Aliphatic matte polyurethane dispersion

Application Characteristics:
1. Increases abrasion resistance and scratch resistance of the finish
2. Film is soft and elastic
3. Excellent mechanical operational stability and leveling
4. Improves overall physical properties, cold resistance, hydrolysis resistance
  
Product Characteristics:
	Appearance
	Milky white liquid

	Solid Content 
	±35%

	pH Value
	7-9




Application Recommendations:
Can be widely used in various leathers, synthetic leather, microfiber (PU, PVC) automotive leather, furniture leather, luggage. The addition of cross-linking agents can improve physical properties.

Storage Method:
Store in sealed original packaging at 5°C ~ 40°C for at least one year. After each use, the packaging should be resealed. Once opened, the product should be used up as soon as possible. This product must be protected from freezing. Must be mixed thoroughly before use.
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